SUMMARY: NESTED | FIELD | | METHOD
DETAIL: FIELD | METHOD

## Class AMT_EthernetPortSettings

Used in features: Intel(R) ME defined Classes

    CIM_ManagedElement
       CIM_SettingData
          AMT_EthernetPortSettings

    class AMT_EthernetPortSettings

extends CIM_SettingData

General Information:
This class contains all Intel(R) AMT specific settings (IP, DHCP) for one network interface in the system.
Qualifiers:
-------------
Version=0.0.3
LOCALE=0x409
dynamic
provider=IntelMEProv
InternalOnly=This class is taken from the ME CIM schema

Supported Fields Summary
`string` | `ElementName` The user-friendly name for this instance of SettingData . . .
`string` | `InstanceID` Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class . . .
`string` | `MACAddress` The MAC address used by Intel(R) AMT in a string format . . .
`boolean` | `LinkIsUp` Indicates whether the network link is up
`boolean` | `DHCPEnabled` Indicates whether DHCP is in use . . .
`string` | `IPAddress` String representation of IP address . . .
`string` | `SubnetMask` Subnet mask in a string format . . .
`string` | `DefaultGateway` Default Gateway in a string format . . .
`string` | `PrimaryDNS` Primary DNS in a string format . . .
`string` | `SecondaryDNS` Secondary DNS in a string format . . .

Methods Summary
`` | `Get(Instance)` Gets the representation of the instance
`` | `Enumerate()` Enumerates the instances of this class

Field Detail

### ElementName

    public string ElementName

  General Information:
  The user-friendly name for this instance of SettingData. In addition, the user-friendly name can be used as an index property for a search or query. (Note: The name does not have to be unique within a namespace.)
  Qualifiers:
  -------------
  Required
  Override=ElementName
  MaxLen=256

### InstanceID

    public string InstanceID

  General Information:
  Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. To ensure uniqueness within the NameSpace, the value of InstanceID should be constructed using the following "preferred" algorithm:
  <OrgID>:<LocalID>
  Where <OrgID> and <LocalID> are separated by a colon (:), and where <OrgID> must include a copyrighted, trademarked, or otherwise unique name that is owned by the business entity that is creating or defining the InstanceID or that is a registered ID assigned to the business entity by a recognized global authority. (This requirement is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness, <OrgID> must not contain a colon (:). When using this algorithm, the first colon to appear in InstanceID must appear between <OrgID> and <LocalID>.
  <LocalID> is chosen by the business entity and should not be reused to identify different underlying (real-world) elements. If the above "preferred" algorithm is not used, the defining entity must assure that the resulting InstanceID is not reused across any InstanceIDs produced by this or other providers for the NameSpace of this instance.
  For DMTF-defined instances, the "preferred" algorithm must be used with the <OrgID> set to CIM.
  Qualifiers:
  -------------
  Key
  Override=InstanceID
  MaxLen=256

### MACAddress

    public string MACAddress

  General Information:
  The MAC address used by Intel(R) AMT in a string format. For Example: 01-02-3f-b0-99-99. (This property can only be read and can't be changed.)
  Qualifiers:
  -------------
  MaxLen=256

### LinkIsUp

    public boolean LinkIsUp

  General Information:
  Indicates whether the network link is up

### DHCPEnabled

    public boolean DHCPEnabled

  General Information:
  Indicates whether DHCP is in use. When this parameter is set to true these parameters will be ignored: SubnetMask, DefaultGAteway, IPAddress, PrimaryDNS, SecondaryDNS.

### IPAddress

    public string IPAddress

  General Information:
  String representation of IP address. Get operation - reports the acquired IP address (whether in static or DHCP mode). Put operation - sets the IP address (in static mode only).
  Qualifiers:
  -------------
  MaxLen=256

### SubnetMask

    public string SubnetMask

  General Information:
  Subnet mask in a string format. For example: 255.255.0.0
  Qualifiers:
  -------------
  MaxLen=256

### DefaultGateway

    public string DefaultGateway

  General Information:
  Default Gateway in a string format. For example: 10.12.232.1
  Qualifiers:
  -------------
  MaxLen=256

### PrimaryDNS

    public string PrimaryDNS

  General Information:
  Primary DNS in a string format. For example: 10.12.232.1
  Qualifiers:
  -------------
  MaxLen=256

### SecondaryDNS

    public string SecondaryDNS

  General Information:
  Secondary DNS in a string format. For example: 10.12.232.1
  Qualifiers:
  -------------
  MaxLen=256

Method Detail

### Get

    public  Get([OUT]AMT_EthernetPortSettings Instance)

  Permission Information:
  No permissions defined
  General Information:
  Gets the representation of the instance

### Enumerate

    public  Enumerate()

  Permission Information:
  All users permitted to use method
  General Information:
  Enumerates the instances of this class

SUMMARY: NESTED | FIELD | METHOD
DETAIL: FIELD | METHOD